;	SERWPL.INF - INF file for USB-to-Serial Device
;	Copyright (C) 2001, Prolific Technology Inc.
;
;	03/14/2001
[Manufacturer]
%Pro%=Pro

[Pro]
%DeviceDesc%=ComPort, USB\VID_067B&PID_2303

[SourceDisksNames]
1=%Pro.Disk%,,,

[SourceDisksFiles]
SER9PL.SYS=1,Win98_ME
SERSPL.VXD=1,Win98_ME
SERSPL.INF=1,Win98_ME
SERWPL.INF=1

[SourceDisksFiles.x86]
ser2pl.sys=1,Win2K

[DestinationDirs]
USB2SER.Files.Ext = 11
USB2SER.Files.Inf = 10,INF
DefaultDestDir=12
ComPort.NT.Copy=12

[ComPort_install]
;Windows98_ME

[Version]
Signature="$Windows 95$"
Class=USB
provider=%Pro%

[PreCopySection]
HKR,,NoSetupUI,,1

[ComPort]
CopyFiles=USB2SER.Files.Ext, USB2SER.Files.Inf
AddReg=USB2SER.AddReg

[USB2SER.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,SER9PL.SYS

[USB2SER.Files.Ext]
SER9PL.SYS
SERSPL.VXD

[USB2SER.Files.Inf]
SERWPL.INF
SERSPL.INF

;========================================================================
;
;========================================================================
[ComPort_Install.NTx86]
;Windows2000

[Version]
Signature="$Windows NT$"
Class=Ports
ClassGuid={4D36E978-E325-11CE-BFC1-08002BE10318}
Provider=%Pro%
LayoutFile=layout.inf
DriverVer=04/09/2002,1.5.0.0

[ComPort.NT]
CopyFiles=ComPort.NT.Copy
AddReg=ComPort.NT.AddReg

[ComPort.NT.HW]
AddReg=ComPort.NT.HW.AddReg

[ComPort.NT.Copy]
ser2pl.sys

[ComPort.NT.AddReg]
HKR,,DevLoader,,*ntkern
HKR,,NTMPDriver,,ser2pl.sys
HKR,,EnumPropPages32,,"MsPorts.dll,SerialPortPropPageProvider"

[ComPort.NT.HW.AddReg]
HKR,,"UpperFilters",0x00010000,"serenum"

[ComPort.NT.Services]
AddService = Ser2pl, 0x00000002, Serial_Service_Inst
AddService = Serenum,,Serenum_Service_Inst

[Serial_Service_Inst]
DisplayName    = %Serial.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_SYSTEM_START (this driver may do detection)
ErrorControl   = 1               ; SERVICE_ERROR_IGNORE
ServiceBinary  = %12%\ser2pl.sys
LoadOrderGroup = Base

[Serenum_Service_Inst]
DisplayName    = %Serenum.SVCDESC%
ServiceType    = 1               ; SERVICE_KERNEL_DRIVER
StartType      = 3               ; SERVICE_DEMAND_START
ErrorControl   = 1               ; SERVICE_ERROR_NORMAL
ServiceBinary  = %12%\serenum.sys
LoadOrderGroup = PNP Filter

[Strings]
Pro = "Prolific"
Pro.Disk = "USB-Serial Cable Diskete"
DeviceDesc = "Prolific USB-to-Serial Comm Port"
Serial.SVCDESC   = "Prolific Serial port driver"
Serenum.SVCDESC = "Serenum Filter Driver"